So they slipped the anchors and left them in the sea, at the same time loosening the linkage that bound the steering oars together. Then they hoisted the foresail to the wind and steered toward the beach.